BCD adder is made using 4-bit adder, which is made using 4 full adders, where each full adder is made using 2 half adders and an XOR gate.

If the output of the 4-bit adder is greater than 9 (i.e. 1001) then 6 (i.e. 0110) is added to it using another 4-bit adder.