4-bit adder is made using four full adders, where each full adder is made using two half adders and an XOR gate.

It takes in two 4-bit numbers as input and produces a 4-bit sum and a carry bit.